<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="-4.5" y1="10.5" x2="8.5" y2="10.5" width="0" layer="20"/>
<wire x1="8.5" y1="10.5" x2="8.5" y2="-2.5" width="0" layer="20"/>
<wire x1="8.5" y1="-2.5" x2="151.5" y2="-2.5" width="0" layer="20"/>
<wire x1="151.5" y1="-2.5" x2="151.5" y2="10.5" width="0" layer="20"/>
<wire x1="151.5" y1="10.5" x2="164.5" y2="10.5" width="0" layer="20"/>
<wire x1="164.5" y1="10.5" x2="164.5" y2="103.5" width="0" layer="20"/>
<wire x1="164.5" y1="103.5" x2="151.5" y2="103.5" width="0" layer="20"/>
<wire x1="151.5" y1="103.5" x2="151.5" y2="116.5" width="0" layer="20"/>
<wire x1="151.5" y1="116.5" x2="8.5" y2="116.5" width="0" layer="20"/>
<wire x1="8.5" y1="116.5" x2="8.5" y2="103.5" width="0" layer="20"/>
<wire x1="8.5" y1="103.5" x2="-4.5" y2="103.5" width="0" layer="20"/>
<wire x1="-4.5" y1="103.5" x2="-4.5" y2="10.5" width="0" layer="20"/>
<hole x="130" y="102" drill="5"/>
<hole x="30" y="102" drill="5"/>
<hole x="80" y="12" drill="5"/>
<text>RS232</text>
<text>ISP</text>
<text>+15V</text>
<text>GND</text>
<text>GND</text>
<text>+5V</text>
<text>BS</text>
<text>LS</text>
<text>BirdView V1.3</text>
<text>(C) Markus Fulde 2012</text>
<text>U1</text>
<text>LM2576 T5</text>
<text>T1</text>
<text>IRLU2905</text>
<text>In1</text>
<text>In2</text>
<text>Out</text>
</plain>
<libraries>
<library name="ConvCtrl">
<packages>
<package name="C050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="0207/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
<package name="DO35-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 10.16 mm</description>
</package>
<package name="MJTP1230">
<description>&lt;b&gt;APEM Kurzhubtaster&lt;/b&gt;</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="HC49U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="E5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 6 mm</description>
</package>
<package name="AKL171-02">
<description>&lt;b&gt;Anreihklemme 2-polig, RM7,5 mm&lt;/b&gt;</description>
</package>
<package name="AKL171-03">
<description>&lt;b&gt;Anreihklemme 3-polig, RM7,5 mm&lt;/b&gt;</description>
</package>
<package name="E5-8,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 8.5 mm</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="TO220-5A">
<description>TO220-5 Package for LM2576&lt;p&gt;
Grid 1,45mm to 1,96 mm
Drill 0,76 mm-1,02 mm</description>
</package>
<package name="C4111-21">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 5.3 mm, horizontal, grid 0.8 inch = 20,32 mm</description>
</package>
<package name="E5-13">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 13 mm</description>
</package>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="C050-030X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 3 x 7.5 mm</description>
</package>
</packages>
</library>
<library name="avr">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL40">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="microchip">
<description>&lt;b&gt;Microchip PIC Microcontrollers and other Devices&lt;/b&gt;&lt;p&gt;
Based on the following sources :
&lt;ul&gt;
&lt;li&gt;Microchip Data Book, 1993
&lt;li&gt;THE EMERGING WORLD STANDARD, 1995/1996
&lt;li&gt;Microchip, Technical Library CD-ROM, June 1998
&lt;li&gt;www.microchip.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
</packages>
</library>
<library name="con-j0011d21b">
<packages>
<package name="J0011D21B">
<description>Ethernet connector J0011D21B PulseJack ( www.pulseeng.com )</description>
</package>
</packages>
</library>
<library name="con-subd">
<description>&lt;b&gt;SUB-D Connectors&lt;/b&gt;&lt;p&gt;
Harting&lt;br&gt;
NorComp&lt;br&gt;
&lt;p&gt;
PREFIX :&lt;br&gt;
H = High density&lt;br&gt;
F = Female&lt;br&gt;
M = Male&lt;p&gt;
NUMBER: Number of pins&lt;p&gt;
SUFFIX :&lt;br&gt;
H = Horizontal&lt;br&gt;
V = Vertical &lt;br&gt;
P = Shield pin on housing&lt;br&gt;
B = No mounting holes&lt;br&gt;
S = Pins individually placeable (Single)&lt;br&gt;
D = Direct mounting &lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="F09HP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-lumberg">
<description>&lt;b&gt;Lumberg Connectors&lt;/b&gt;&lt;p&gt;
include con-mfs.lbr - 2001.03.22&lt;br&gt;
Jack connectors - 2005.11.23&lt;p&gt;
http://www.lumberg.de&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="WBTOR1">
<description>&lt;b&gt;RCA connectors according to JEITA RC-5231&lt;/b&gt; Cinch&lt;p&gt;
RCA-Einbaukupplung nach JEITA RC-5231, abgewinkelte Ausführung&lt;br&gt;
Source: http://www.lumberg.de/Produkte/PDFs/WBTOR1.pdf</description>
</package>
</packages>
</library>
<library name="connectors">
<description>&lt;table width="100%" cellpadding="5" cellspacing="0"  bgcolor="#E0E0E0"&gt;
&lt;tr&gt;&lt;td&gt;
&lt;b&gt;Connectors&lt;/b&gt;&lt;br&gt;
Connectors, screw + crimp terminals, jumpers, test points, pins, pads, ...&lt;br&gt;
&lt;author&gt;&lt;b&gt;Update:&lt;/b&gt; 2009-07-02 Andreas Weidner&lt;/author&gt;
&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;
&lt;br&gt;

&lt;b&gt;Device prefixes&lt;/b&gt;&lt;br&gt;
All devices have a dedicated prefix, sometimes followed by a 2-digit number, which signify
the connector type and its pin number. The following device types are available (excerpt):&lt;p&gt;
&lt;table border="0" cellpadding="0" cellspacing="0"&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;J[Nr]&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Jumper [length in 0.1"]&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;JP[Nr]&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Jumper pin block [pin number]&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;X[Nr]&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Connector [pin number]&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XA[Nr]&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Connector with alternating pins [pin number]&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XB[Nr]&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Backplane connector [pin number]&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XC&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Crimp terminal for shielded cables&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XD&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Digital ground test point&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XG&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Ground test point&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XP&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Input/output pin&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XS&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Shielded connector&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XT&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Test point&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XU[Nr]&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Connector with unconnected (separate) pins [pin number]&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;hr&gt;

&lt;b&gt;Connector suffixes&lt;/b&gt;&lt;br&gt;
Most connectors offer different suffixes to directly specify the package type. The following list gives some
examples of available suffixes (note that not all connectors offer all types of packages):&lt;p&gt;
&lt;table border="0" cellpadding="0" cellspacing="0"&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;(none)&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Default connector package (currently DIL with normal pads, if available)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;D&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;DIL package with normal pads (easily solderable)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;DR&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;DIL package with reduced pads (small, through-pin-routing possible)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;I&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;IDC package with normal pads (easily solderable)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;IR&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;IDC package with reduced pads (small, through-pin-routing possible)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;L&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;SIL package with long pads (easily solderable, through-pin-routing possible)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;N&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;SIL package with normal pads (easily solderable)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;R&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;SIL package with reduced pads (small, through-pin-routing possible)&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;hr&gt;

&lt;b&gt;Pin suffixes&lt;/b&gt;&lt;br&gt;
Most input/output pins offer different suffixes to directly specify the pad type. The following suffixes
are available (note that not all pins offer all types of pads):&lt;p&gt;
&lt;table border="0" cellpadding="0" cellspacing="0"&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;N &lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Normal pad (easily solderable)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;L &lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Long pad (easily solderable, through-pin-routing possible)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;R &lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Reduced pad (small, through-pin-routing possible)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;B &lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Big pad (0.1")&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;H &lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Huge pad (0.15")&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;M &lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Maximised pad (0.2")&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;hr&gt;

&lt;b&gt;Device examples&lt;/b&gt;&lt;br&gt;
The following examples show devices that can be inserted into EAGLE schematics using
the &lt;b&gt;add&lt;/b&gt; command:&lt;p&gt; 
&lt;table border="0" cellpadding="0" cellspacing="0"&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;J&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Default jumper (currently 0.2" with normal pads)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;X06&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Default 6-pin connector (currently DIL package with normal pads)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XA16IR&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;16-pin connector with alternating pins in IDC package with reduced pads&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XC&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Default crimp terminal for shielded cables&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XPL&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Input/output pin with long pads&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;hr&gt;

&lt;b&gt;Board layers&lt;/b&gt;&lt;br&gt;
The board packages make special use of the following layers:&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;tPlace,&lt;br&gt;&amp;nbsp;tNames,&lt;br&gt;&amp;nbsp;tValues&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Placeplan including device names and values for printed documentation. Should
    &lt;b&gt;not&lt;/b&gt; be used for the board imprint due to complexity. Names and values occupy
    the &lt;b&gt;same&lt;/b&gt; board space, so two separate printouts are advisable&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;tDocu&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Less sophisticated, but concise placeplan with device names for the board imprint&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="XS-BNC01L">
<description>&lt;b&gt;BNC connector&lt;/b&gt;, angled, with long pads&lt;br&gt;
Connector mounting hole 12.5mm, center 8.2mm above PCB surface</description>
</package>
</packages>
</library>
<library name="uln-udn">
<description>&lt;b&gt;Driver Arrays&lt;/b&gt;&lt;p&gt;
ULN and UDN Series&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="relay_finder">
<description>Library for the FINDER relay P.C.B. sockets 95.15.2 &amp; 94.13.0
www.findernet.com

by Arkoudouperman
aristosk@hotmail.com</description>
<packages>
<package name="43.41">
<description>Package für Finer Relais 43.41.7.005.2000&lt;br&gt;
5V / 10A / 250V~</description>
</package>
</packages>
</library>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="317TS">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor-npn">
<description>&lt;b&gt;NPN Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92-EBC">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
 grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="transistor-power">
<description>&lt;b&gt;Power Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO-251AA">
<description>TO-251AA 
&lt;p&gt;www.irf.com
&lt;p&gt;IRLR2905.pdf</description>
</package>
</packages>
</library>
<library name="mf-transistor-power">
<description>&lt;b&gt;Power Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220AV">
<description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="switch-omron">
<description>&lt;b&gt;Omron Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B3F-31XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="inductor-fastron">
<description>&lt;b&gt;Fastron Inductors&lt;/b&gt;&lt;p&gt;
&lt;author&gt; created by S.Essig@gmx.net &lt;/author&gt;</description>
<packages>
<package name="PIS4728">
</package>
</packages>
</library>
<library name="con-harting-ml">
<description>&lt;b&gt;Harting  &amp; 3M Connectors&lt;/b&gt;&lt;p&gt;
Low profile connectors, straight&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="ML6">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
<package name="ML10">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="relay">
<description>&lt;b&gt;Relays&lt;/b&gt;&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;Eichhoff
&lt;li&gt;Finder
&lt;li&gt;Fujitsu
&lt;li&gt;HAMLIN
&lt;li&gt;OMRON
&lt;li&gt;Matsushita
&lt;li&gt;NAiS
&lt;li&gt;Siemens
&lt;li&gt;Schrack
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="G5V-2">
<description>&lt;b&gt;OMRON PCB Relay&lt;/b&gt;&lt;p&gt;
Source: http://www.omron.com/ecb/products/pdf/en-g5v2.pdf</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C8" library="ConvCtrl" package="C050-025X075" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="ConvCtrl" package="0207/12" value="10µH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="ConvCtrl" package="DO35-10" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="ConvCtrl" package="MJTP1230" value="Reset">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="ConvCtrl" package="0207/10" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="ConvCtrl" package="C050-025X075" value="47nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="ConvCtrl" package="C050-025X075" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="avr" package="DIL40" value="MEGA32-P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="ConvCtrl" package="C025-024X044" value="22pF"/>
<element name="C6" library="ConvCtrl" package="C025-024X044" value="22pF"/>
<element name="Q1" library="ConvCtrl" package="HC49U-V" value="16 MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="ConvCtrl" package="C050-025X075" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="microchip" package="DIL28-3" value="ENC28J60SP">
<attribute name="OC_NEWARK" value="96K3661"/>
<attribute name="MPN" value="ENC28J60/SP"/>
<attribute name="MF" value="MICROCHIP"/>
<attribute name="OC_FARNELL" value="1084619"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JACK" library="con-j0011d21b" package="J0011D21B" value="TRJ0011BANL"/>
<element name="R13" library="ConvCtrl" package="0207/10" value="2k2"/>
<element name="C13" library="ConvCtrl" package="E5-6" value="100µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="ConvCtrl" package="C025-024X044" value="22pF"/>
<element name="C14" library="ConvCtrl" package="C025-024X044" value="22pF"/>
<element name="Q2" library="ConvCtrl" package="HC49U-V" value="25 MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="ConvCtrl" package="0207/10" value="220R"/>
<element name="R6" library="ConvCtrl" package="0207/10" value="220R"/>
<element name="R9" library="ConvCtrl" package="0207/10" value="51R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="ConvCtrl" package="0207/10" value="51R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="ConvCtrl" package="0207/10" value="51R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="ConvCtrl" package="0207/10" value="51R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="ConvCtrl" package="C050-025X075" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="ConvCtrl" package="C050-025X075" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="ConvCtrl" package="0207/12" value="10µH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="ConvCtrl" package="0207/10" value="3k3"/>
<element name="X2" library="con-subd" package="F09HP" value="SUBD-9 Female">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="con-lumberg" package="WBTOR1" value="Audio">
<attribute name="OC_NEWARK" value="98K2588"/>
<attribute name="MPN" value="WBTOR 1 BLACK"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1200146"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X4" library="connectors" package="XS-BNC01L" value="Video1-In">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X5" library="connectors" package="XS-BNC01L" value="Video2-In">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X7" library="connectors" package="XS-BNC01L" value="Video-Out">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X8" library="ConvCtrl" package="AKL171-02" value="+15V Betriebsspannung">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="uln-udn" package="DIL16" value="ULN2003AN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="ConvCtrl" package="C050-025X075" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="K1" library="relay_finder" package="43.41" value="Finser Relais 43.41 5V"/>
<element name="D3" library="ConvCtrl" package="DO35-10" value="1N4148"/>
<element name="X3" library="ConvCtrl" package="AKL171-03" value="Wechselschalter">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="v-reg" package="317TS" value="LM317"/>
<element name="C1" library="ConvCtrl" package="E5-8,5" value="100µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="ConvCtrl" package="E5-6" value="100µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="ConvCtrl" package="0207/10" value="1k5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="ConvCtrl" package="LED3MM" value="3mm LC grün">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="ConvCtrl" package="0207/10" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="ConvCtrl" package="0207/10" value="270R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="ConvCtrl" package="LED3MM" value="3mm LC grün">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="ConvCtrl" package="0207/10" value="698R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="ConvCtrl" package="0207/10" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="transistor-npn" package="TO92-EBC" value="BC548">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="ConvCtrl" package="0207/10" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="ConvCtrl" package="0207/10" value="0R0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="ConvCtrl" package="0207/10" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="ConvCtrl" package="0207/10" value="100R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q6" library="transistor-npn" package="TO92-EBC" value="BC548">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="ConvCtrl" package="0207/10" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="ConvCtrl" package="0207/10" value="0R0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="ConvCtrl" package="0207/10" value="1k"/>
<element name="R21" library="ConvCtrl" package="0207/10" value="100R"/>
<element name="T1" library="transistor-power" package="TO-251AA" value="IRLU2905"/>
<element name="R26" library="ConvCtrl" package="0207/10" value="250R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="ConvCtrl" package="0207/10" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="mf-transistor-power" package="TO220AV" value="IRF5305"/>
<element name="Q5" library="mf-transistor-power" package="TO220AV" value="IRF5305"/>
<element name="S3" library="switch-omron" package="B3F-31XX" value="Taste 2">
<attribute name="OC_NEWARK" value="36M3582"/>
<attribute name="MPN" value="B3F-3100"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="959704"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="ConvCtrl" package="0207/10" value="1k5"/>
<element name="LED6" library="ConvCtrl" package="LED3MM" value="LC 3mm grün">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="ConvCtrl" package="0207/10" value="1k5"/>
<element name="LED7" library="ConvCtrl" package="LED3MM" value="LC 3mm yellow">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="ConvCtrl" package="LED3MM" value="LC 3mm rot">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="ConvCtrl" package="0207/10" value="1k5"/>
<element name="R18" library="ConvCtrl" package="0207/10" value="6k5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="ConvCtrl" package="0207/10" value="6k5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="ConvCtrl" package="LED3MM" value="LC 3mm grün">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="ConvCtrl" package="LED3MM" value="LC 3mm grün">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="ConvCtrl" package="0207/10" value="1k5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED8" library="ConvCtrl" package="LED3MM" value="LC 3mm rot">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED9" library="ConvCtrl" package="LED3MM" value="LC 3mm rot"/>
<element name="LED10" library="ConvCtrl" package="LED3MM" value="LC 3mm rot"/>
<element name="R34" library="ConvCtrl" package="0207/10" value="1k5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="ConvCtrl" package="0207/10" value="1k5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="switch-omron" package="B3F-31XX" value="Taste 1">
<attribute name="OC_NEWARK" value="36M3582"/>
<attribute name="MPN" value="B3F-3100"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="959704"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S4" library="switch-omron" package="B3F-31XX" value="Taste 3">
<attribute name="OC_NEWARK" value="36M3582"/>
<attribute name="MPN" value="B3F-3100"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="959704"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="ConvCtrl" package="0207/10" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="ConvCtrl" package="0207/10" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="ConvCtrl" package="0207/10" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="ConvCtrl" package="0207/10" value="8450R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="ConvCtrl" package="TO220-5A" value="LM2576T-5"/>
<element name="D1" library="ConvCtrl" package="C4111-21" value="1N5821">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="ConvCtrl" package="E5-13" value="1000µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="inductor-fastron" package="PIS4728" value="100µH"/>
<element name="JP1" library="ConvCtrl" package="JP1" value="VCC_Select"/>
<element name="X6" library="ConvCtrl" package="AKL171-02" value="+5V Betriebspannung (extern)">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="ConvCtrl" package="C050-030X075" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="ConvCtrl" package="0207/10" value="1k5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED11" library="ConvCtrl" package="LED3MM" value="LC 3mm grün">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SV1" library="con-harting-ml" package="ML6" value="ISP6">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="SV2" library="con-harting-ml" package="ML10" value="RS232">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="K2" library="relay" package="G5V-2" value="G5V-2">
<attribute name="OC_NEWARK" value="78K5703"/>
<attribute name="MPN" value="G5V-2 5DC"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9949488"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T2" library="transistor" package="TO92" value="BC337">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED12" library="ConvCtrl" package="LED3MM" value="LC gelb 3mm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="ConvCtrl" package="0207/10" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="ConvCtrl" package="DO35-10" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="ConvCtrl" package="0207/10" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="X2" pad="2"/>
<contactref element="X2" pad="4"/>
<contactref element="X1" pad="S"/>
<contactref element="X7" pad="GND"/>
<contactref element="X5" pad="GND"/>
<contactref element="X4" pad="GND"/>
<contactref element="X6" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="C4" pad="-"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="IC2" pad="11"/>
<contactref element="IC2" pad="31"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="S1" pad="3"/>
<contactref element="C9" pad="2"/>
<contactref element="S1" pad="4"/>
<contactref element="C10" pad="2"/>
<contactref element="IC3" pad="11"/>
<contactref element="IC3" pad="2"/>
<contactref element="IC3" pad="18"/>
<contactref element="IC3" pad="21"/>
<contactref element="IC3" pad="22"/>
<contactref element="R13" pad="2"/>
<contactref element="C13" pad="-"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="JACK" pad="GND"/>
<contactref element="JACK" pad="G_GND"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="IC4" pad="8"/>
<contactref element="C16" pad="2"/>
<contactref element="R19" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="Q4" pad="E"/>
<contactref element="R23" pad="1"/>
<contactref element="Q6" pad="E"/>
<contactref element="T1" pad="3"/>
<contactref element="R27" pad="1"/>
<contactref element="LED3" pad="K"/>
<contactref element="LED4" pad="K"/>
<contactref element="S2" pad="1"/>
<contactref element="S3" pad="1"/>
<contactref element="S4" pad="1"/>
<contactref element="R37" pad="1"/>
<contactref element="SV1" pad="6"/>
<contactref element="SV2" pad="9"/>
<contactref element="C1" pad="-"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="D1" pad="A"/>
<contactref element="C3" pad="-"/>
<contactref element="C2" pad="2"/>
<contactref element="X8" pad="2"/>
<contactref element="JACK" pad="Y"/>
<contactref element="T2" pad="1"/>
</signal>
<signal name="+15V1">
<contactref element="X2" pad="1"/>
<contactref element="Q3" pad="C"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="+15V2">
<contactref element="X2" pad="3"/>
<contactref element="Q5" pad="C"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="IR_GND">
<contactref element="X2" pad="6"/>
<contactref element="T1" pad="2"/>
</signal>
<signal name="AUDIO">
<contactref element="X2" pad="7"/>
<contactref element="X1" pad="T"/>
</signal>
<signal name="VCC">
<contactref element="X2" pad="8"/>
<contactref element="X6" pad="1"/>
<contactref element="C4" pad="+"/>
<contactref element="LED1" pad="A"/>
<contactref element="IC1" pad="3"/>
<contactref element="JP1" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="IC2" pad="32"/>
<contactref element="IC2" pad="10"/>
<contactref element="L2" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="C10" pad="1"/>
<contactref element="IC4" pad="9"/>
<contactref element="C16" pad="1"/>
<contactref element="K1" pad="A1"/>
<contactref element="D3" pad="C"/>
<contactref element="R25" pad="2"/>
<contactref element="R28" pad="1"/>
<contactref element="R32" pad="1"/>
<contactref element="R33" pad="1"/>
<contactref element="R34" pad="1"/>
<contactref element="R35" pad="1"/>
<contactref element="R29" pad="2"/>
<contactref element="R30" pad="2"/>
<contactref element="R31" pad="2"/>
<contactref element="R36" pad="1"/>
<contactref element="SV1" pad="2"/>
<contactref element="SV2" pad="10"/>
<contactref element="K2" pad="1"/>
<contactref element="R38" pad="2"/>
<contactref element="D4" pad="C"/>
</signal>
<signal name="LDR">
<contactref element="X2" pad="9"/>
<contactref element="IC2" pad="40"/>
<contactref element="R37" pad="2"/>
</signal>
<signal name="VIDEO1-IN">
<contactref element="X4" pad="SIG"/>
<contactref element="K2" pad="6"/>
</signal>
<signal name="VIDEO2-IN">
<contactref element="X5" pad="SIG"/>
<contactref element="K2" pad="8"/>
</signal>
<signal name="VIDEO-OUT">
<contactref element="X7" pad="SIG"/>
<contactref element="K2" pad="4"/>
</signal>
<signal name="+15V">
<contactref element="X8" pad="1"/>
<contactref element="R14" pad="2"/>
<contactref element="Q3" pad="E"/>
<contactref element="R20" pad="2"/>
<contactref element="Q5" pad="E"/>
<contactref element="C1" pad="+"/>
<contactref element="U1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="RELAIS_12">
<contactref element="X3" pad="1"/>
<contactref element="K1" pad="12"/>
</signal>
<signal name="RELAIS_11">
<contactref element="K1" pad="11"/>
<contactref element="X3" pad="3"/>
</signal>
<signal name="RELAIS_14">
<contactref element="K1" pad="14"/>
<contactref element="X3" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="LED1" pad="K"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="LED2" pad="K"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="LED2" pad="A"/>
<contactref element="IC3" pad="28"/>
<contactref element="IC3" pad="19"/>
<contactref element="IC3" pad="20"/>
<contactref element="IC3" pad="25"/>
<contactref element="IC3" pad="15"/>
<contactref element="L3" pad="1"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$33">
<contactref element="U1" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="L1" pad="P$1"/>
</signal>
<signal name="VCC_1">
<contactref element="U1" pad="4"/>
<contactref element="L1" pad="P$2"/>
<contactref element="C3" pad="+"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="XTAL2">
<contactref element="C5" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="XTAL1">
<contactref element="C6" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="RESET">
<contactref element="IC2" pad="9"/>
<contactref element="R5" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="SV1" pad="5"/>
</signal>
<signal name="AVCC">
<contactref element="IC2" pad="30"/>
<contactref element="L2" pad="2"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="IC2" pad="8"/>
<contactref element="IC3" pad="8"/>
<contactref element="SV1" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="IC2" pad="7"/>
<contactref element="IC3" pad="6"/>
<contactref element="SV1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="IC2" pad="6"/>
<contactref element="IC3" pad="7"/>
<contactref element="SV1" pad="4"/>
</signal>
<signal name="TXD">
<contactref element="IC2" pad="15"/>
<contactref element="SV2" pad="1"/>
</signal>
<signal name="RXD">
<contactref element="IC2" pad="14"/>
<contactref element="SV2" pad="2"/>
</signal>
<signal name="CS">
<contactref element="IC2" pad="5"/>
<contactref element="IC3" pad="9"/>
</signal>
<signal name="INT">
<contactref element="IC2" pad="17"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="RELAIS">
<contactref element="IC2" pad="33"/>
<contactref element="IC4" pad="1"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="PWR_CAM2">
<contactref element="IC2" pad="34"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="PWR_CAM1">
<contactref element="IC2" pad="35"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="IR_PWM">
<contactref element="IC2" pad="21"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="VIDEO_SHDN">
<contactref element="IC2" pad="23"/>
</signal>
<signal name="VIDEO_SEL">
<contactref element="IC2" pad="22"/>
<contactref element="R39" pad="1"/>
</signal>
<signal name="ALIVE_LED">
<contactref element="IC4" pad="2"/>
<contactref element="IC2" pad="29"/>
</signal>
<signal name="ENC_LED">
<contactref element="IC4" pad="3"/>
<contactref element="IC2" pad="28"/>
</signal>
<signal name="IR_LED">
<contactref element="IC4" pad="4"/>
<contactref element="IC2" pad="27"/>
</signal>
<signal name="VIDEO1_LED">
<contactref element="IC4" pad="5"/>
<contactref element="IC2" pad="26"/>
</signal>
<signal name="VIDEO2_LED">
<contactref element="IC4" pad="6"/>
<contactref element="IC2" pad="25"/>
</signal>
<signal name="KEY1">
<contactref element="IC2" pad="1"/>
<contactref element="S2" pad="2"/>
<contactref element="R29" pad="1"/>
</signal>
<signal name="KEY2">
<contactref element="IC2" pad="2"/>
<contactref element="S3" pad="2"/>
<contactref element="R30" pad="1"/>
</signal>
<signal name="KEY3">
<contactref element="IC2" pad="3"/>
<contactref element="S4" pad="2"/>
<contactref element="R31" pad="1"/>
</signal>
<signal name="MODE_LED">
<contactref element="IC4" pad="7"/>
<contactref element="IC2" pad="24"/>
</signal>
<signal name="RBIAS">
<contactref element="IC3" pad="14"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="VCAP">
<contactref element="C13" pad="+"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="OSC2">
<contactref element="C15" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="IC3" pad="24"/>
</signal>
<signal name="OSC1">
<contactref element="C14" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="IC3" pad="23"/>
</signal>
<signal name="N$5">
<contactref element="IC3" pad="17"/>
<contactref element="JACK" pad="TD+"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="IC3" pad="16"/>
<contactref element="JACK" pad="TD-"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC3" pad="13"/>
<contactref element="JACK" pad="RD+"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC3" pad="12"/>
<contactref element="JACK" pad="RD-"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="L3" pad="2"/>
<contactref element="JACK" pad="CT"/>
</signal>
<signal name="N$10">
<contactref element="R12" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R7" pad="1"/>
<contactref element="JACK" pad="G"/>
</signal>
<signal name="N$2">
<contactref element="R6" pad="1"/>
<contactref element="JACK" pad="Y_GND"/>
</signal>
<signal name="N$3">
<contactref element="IC3" pad="27"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="IC3" pad="26"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="R8" pad="1"/>
<contactref element="IC3" pad="10"/>
</signal>
<signal name="RELAIS_GND">
<contactref element="IC4" pad="16"/>
<contactref element="K1" pad="A2"/>
<contactref element="D3" pad="A"/>
<contactref element="LED5" pad="K"/>
</signal>
<signal name="N$14">
<contactref element="R16" pad="2"/>
<contactref element="Q4" pad="B"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="R14" pad="1"/>
<contactref element="Q4" pad="C"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="R15" pad="2"/>
<contactref element="Q3" pad="B"/>
</signal>
<signal name="N$13">
<contactref element="R22" pad="2"/>
<contactref element="Q6" pad="B"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="R20" pad="1"/>
<contactref element="Q6" pad="C"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="R21" pad="2"/>
<contactref element="Q5" pad="B"/>
</signal>
<signal name="N$22">
<contactref element="R26" pad="2"/>
<contactref element="T1" pad="1"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="ALIVE_GND">
<contactref element="IC4" pad="15"/>
<contactref element="LED6" pad="K"/>
</signal>
<signal name="ENC_GND">
<contactref element="IC4" pad="14"/>
<contactref element="LED7" pad="K"/>
</signal>
<signal name="N$27">
<contactref element="R25" pad="1"/>
<contactref element="LED5" pad="A"/>
</signal>
<signal name="N$29">
<contactref element="LED4" pad="A"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="LED3" pad="A"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="IR_LED_GND">
<contactref element="IC4" pad="13"/>
<contactref element="LED8" pad="K"/>
</signal>
<signal name="VIDEO1_GND">
<contactref element="IC4" pad="12"/>
<contactref element="LED9" pad="K"/>
</signal>
<signal name="VIDEO2_GND">
<contactref element="IC4" pad="11"/>
<contactref element="LED10" pad="K"/>
</signal>
<signal name="MODE_GND">
<contactref element="IC4" pad="10"/>
<contactref element="LED11" pad="K"/>
</signal>
<signal name="N$24">
<contactref element="R28" pad="2"/>
<contactref element="LED6" pad="A"/>
</signal>
<signal name="N$26">
<contactref element="R32" pad="2"/>
<contactref element="LED7" pad="A"/>
</signal>
<signal name="N$28">
<contactref element="R33" pad="2"/>
<contactref element="LED8" pad="A"/>
</signal>
<signal name="N$31">
<contactref element="R34" pad="2"/>
<contactref element="LED9" pad="A"/>
</signal>
<signal name="N$32">
<contactref element="R35" pad="2"/>
<contactref element="LED10" pad="A"/>
</signal>
<signal name="N$34">
<contactref element="R36" pad="2"/>
<contactref element="LED11" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="R39" pad="2"/>
<contactref element="T2" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="R38" pad="1"/>
<contactref element="LED12" pad="A"/>
</signal>
<signal name="N$25">
<contactref element="K2" pad="16"/>
<contactref element="LED12" pad="K"/>
<contactref element="D4" pad="A"/>
<contactref element="T2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
